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Off Farm Manure Supplier Affidavit
Operation Name: __________________________________________________________
Supplier Name: ___________________________________________________________
Please have the supplier of the Manure provide the following information:

· Manure is from  FORMCHECKBOX 
 Cattle    FORMCHECKBOX 
 Horses    FORMCHECKBOX 
Poultry    FORMCHECKBOX 
 Other:_____________

· Type of Operation the manure is coming from:   FORMCHECKBOX 
 Organic   FORMCHECKBOX 
 Conventional
· Form manure is supplied in:  FORMCHECKBOX 
 Solid    FORMCHECKBOX 
 Liquid    FORMCHECKBOX 
 Pelleted    FORMCHECKBOX 
 Semi-Solid              
 FORMCHECKBOX 
 Dehydrated      FORMCHECKBOX 
 Other:___________________________

· Are there additives added to the manure?    FORMCHECKBOX 
 Yes    FORMCHECKBOX 
 No

If yes, please list what is added:___________________________________

Please provide supporting documentation for all additives (Label, SDS, Tech Sheet, etc.) as applicable.

At what stage are the additives incorporated to the manure? 

 FORMCHECKBOX 
 Before it is piled for sale

 FORMCHECKBOX 
 After it is piled for sale 

 FORMCHECKBOX 
 Other: _________________________________

· Does the manure contain sewage sludge?   FORMCHECKBOX 
 Yes    FORMCHECKBOX 
No

· Is the manure composted?    FORMCHECKBOX 
 Yes    FORMCHECKBOX 
 No

If yes, does the composting process comply with the following requirements of Composting, as defined in 205.2 of the NOP Rule, see below?  FORMCHECKBOX 
 Yes    FORMCHECKBOX 
 No
Compost. The product of a managed process through which microorganisms break down plant and animal materials into more available forms suitable for application to the soil. Compost must be produced through a process that combines plant and animal materials with an initial C:N ratio of between 25:1 and 40:1. Producers using an in-vessel or static aerated pile system must maintain the composting materials at a temperature between 131 °F and 170 °F for 3 days. Producers using a windrow system must maintain the composting materials at a temperature between 131 °F and 170 °F for 15 days, during which time, the materials must be turned a minimum of five times.
 FORMCHECKBOX 
 I, ___________________ (Supplier of the manure), hereby attest that all of the above and attached information is true and correct. 

Manure Supplier

____________________________________                                     _____________________
Signature of Authorized Representative                                              Date
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